Wind span:

The wind span is that on which the wind is assumed to act transversely on the conductors and is taken as half the sum of the two spans, adjacent to the support.

Weight span:

The weight span is the horizontal distance between the lowest points of the conductors, on the two spans adjacent to the tower



